Mixes two wireless networks each on their
own radio frequency and each of size 3
nodes (0,1,2) and (3,4,5).  Nodes 0 and
3 are connected by a point to point link.
A static routing file "mixed_rtable.in"
is used for routes (see topology
diagram in that file).




